Product/Accessory Part Numbers:	P766256:	ACME SpeedPrint 1440
C835285:	Black ink cartridge
C835286:	Color ink cartridge	
Printing Method	Four color (CMYK) ink jet technology	
Nozzle Configuration	Monochrome Head: 128 nozzles
Color Head: 64 nozzles x 3 (CMY)	
Resolution	1440 x 1440 dpi; 720 x 720 dpi; 360 x 360 dpi; 180 x 180 dpi	
Print Speed	Maximum engine rated print speeds up to 10 PPM monochrome; 8 PPM color.	
Sound Level	45 dB(A) (ISO 7779)	
Dimensions (W x D x H)	26" x 19.4" x 7.7"
24.8 lbs.	
Input Buffer	64 Kb	
Interface	Bi-directional parallel interface (IEEE-1284)	
Printable Area	8.26" x 10.34" (letter size)
Top margin: .12"
Left margin: .12"
Right margin: .12"
Bottom margin: .54"	
Paper Capacity	Input paper tray: 100 sheets/ 10 envelopes
Output paper tray: 30 sheets	
Paper handling	Single sheets: Letter, legal, A5, A4, A3, B5, executive, statement, user definable
Thickness: .0025" to .004"
Weight: 17 to 24 lbs.	
Environmental Characteristics
Temperature:

Humidity:	

Operating: 50° to 95° F (10° to 35° C)
Storage: -4° to 140° F (-20° to 60° C)

Operating: 20 to 80% relative humidity
Storage: 5 to 85% relative humidity (no condensation)	
Safety Approvals	Safety Standards:
UL1950 with D3
CSA22.2 950 with D3
EMI FCC Part 15 subpart B class B	
Reliability
Print head life:

Total print volume:	
2000 million dots/nozzle (color and monochrome)
75,000 pages (A3)	
Electrical Requirements
Rated voltage:
Rated frequency:
Rated current:
Power consumption:	
120V AC +/- 10%
50 to 60 Hz
0.4 A
Approx. 21W (ISO/IEC 10561 Letter Pattern)	
Ink Cartridge Life
Black ink life:
Color ink life:

Shelf life:	
1000 pages at 5% coverage
320 pages at 15% coverage (5% each cyan, magenta, yellow)
2 years from production	
Warranty	Two year limited	
Support:
ACME Automated Support
ACME Download Service
Pre-Sales Support
Internet Website	
800-226-2886
800-226-3537
800-226-7725
http://www.acmeprinters.com