Product/Accessory Part Numbers:	P766249:	ACME SpeedPrint 720
C835285:	Black ink cartridge
C835286: 	Color ink cartridge	
Printing Method	Four color (CMYK) ink jet technology	
Nozzle Configuration	Monochrome Head: 64 nozzles
Color Head: 21 nozzles x 3 (CMY)	
Resolution	720 x 720 dpi; 360 x 360 dpi; 180 x 180 dpi	
Sound Level	45 dB(A)	
Dimensions (W x D x H)	18.9" x 9.4" x 6.7"
11.8 lbs.	
Input Buffer	10 Kb	
Interface	8-bit bi-directional parallel interface (IEEE-1284)	
Printable Area	8.26" x 10.34" (letter size)
Top margin: .12"
Left margin: .12"
Right margin: .12"
Bottom margin: .54"	
Paper Capacity	Input paper tray: 100 sheets/ 10 envelopes
Output paper tray: 30 sheets	
Paper handling	Single sheets: Letter, legal, A4, B5, executive, statement, user definable
Thickness: .003" to .004"
Weight: 17 to 24 lbs.	
Environmental Characteristics	Temperature:
Operating: 50° to 95° F (10° to 35° C)
Storage: -4° to 140° F (-20° to 60° C)
Humidity:
Operating: 20 to 80% relative humidity
Storage: 5 to 85% relative humidity (no condensation)	
Safety Approvals	Safety Standards:
UL1950 with D3
CSA22.2 950 with D3
R.F.I. FCC Part 15 subpart B class B
CSA C108.8 class B	
Reliability	Print head life: 2000 million dots/nozzle (color and monochrome)
Total print volume: 10,000 pages (letter or A4)	
Electrical Requirements	Rated voltage: 120V AC +/- 10%
Rated frequency: 50 to 60 Hz
Rated current: 0.4 Amp (Maximum)
Power consumption: Approx. 15W (self test mode)	
Ink Cartridge Life	Black ink life: 540 pages at 5% coverage
Color ink life: 300 pages at 15% coverage (5% each cyan, magenta, yellow)
Shelf life: 2 years from production	
Warranty	One year limited	
Support:
ACME Automated Support
ACME Download Service
Pre-Sales Support
Internet Website	
800-226-2886
800-226-3537
800-226-7725
http://www.acmeprinters.com